Tool List - Electrician Following are the tool requirements for each electrician when hired: (1) Tape Measure - 25' (R) (1) 9" Pliers (R) (1) Dikes (R) (1) Needle Nose Pliers (R) (1) Knife (R) (2) Phillips Screw Drivers (R) (1) Wire Strippers / Screw Cutter Pliers (P) (2) Regular Screw Drivers (R) (1) Claw Hammer (R) (1) Flashlight (P) (1) Set End Wrenches 7/16-3/4 (P) (1) Battery operated 1/2" Drill (1) Sawzall (P) (1) 1/2" Drill 120v w/cord (P) (1) Drill Index 1/8-1/2 (P) (1) Hole Hawg (P) (1) Amprobe / Voltmeter(P) (1) Hacksaw (R) (1) Keyhole Saw (P) (1) 6", 8", 12" Crescent Wrenches (P) (1) Socket Set 1/4-3/4 (P) (1) Set Left & Right Hand Aviation/Tin Snips (P) (1) Channel Locks Pliers (R) (1) 6-32 and 8-3 Z-Taps (P) (1) Chain Wrench (P) (1) 4' Level (P) (1) Torpedo Level (R) (1) Drop Light (P) (1) Tool Pouch (R) (1) Set Benders 1/2", 3/4", 1" is Preferred (R) R=Required P=Preferred that you have Policy No. 581